Simulation Parameters

(Simulation Menu)

- The default extraction includes the removal of redundant boxes (Purge) and the removal of overlaps (Merge). The fast extraction does not handle Purge nor Merge operations.

- The MOS level can be chosen between level 1,3 and BSIM4. See the user's manual for more details about those models.

- Other options concern the computation of lateral capacitance and vertical crosstalk capacitance.
- The temperature may be changed in this screen.

[Back]